Goundwire setup for webconnex.
See the last 2 pages for QR codes

|  |  |
| --- | --- |
|  | Tap the menu icon (3 dots, top right) |
|  | Under Notifications, tap Incoming Calls and select Push Notifications.This is important because it saves battery and allows incoming calls when the phone is asleep.When done, tap Accounts |
|  | Tap **+** to add a new account (bottom right)In this screenshot I already have the account for webconnex so I would tap that. |
|  | Give the account a TitleEG. webconnex or WorkUsername: (provided by admin)Password: (provided by admin)Next, tap Advanced Settings |
|  | Tap **Codec for Wi-Fi**Set these Codecs You can drag them around with the handle that looks like =Tap the back icon when done (Top left) |
|  | Tap **Codec for Mobile Data**Set these CodecsYou can drag them around with the handle that looks like =Tap the back icon when done (Top left) |
|  | Tap **Video codec for Wi-Fi**Set these CodecsYou can drag them around with the handle that looks like =Tap the back icon when done (Top left) |
|  | Tap **Video codec for Mobile Data**Set these CodecsYou can drag them around with the handle that looks like =Tap the back icon when done (Top left) |
|  | Swipe up to see these settingsEnable **Call Waiting** (so you done miss a call)Set the **Transport Protocol** to **tls (sips)** |
|  | Tap DTMF ModeThis is used for responding to auto attendant menus (Dial 1 for this, dial 2 for that, etc.)You can drag them around with the handle that looks like =Tap the back icon when done (Top left) |
|  | Tap **Secure Calls**Note: External calls are **always** insecure.You can enable these for incoming and outgoingTap the back icon when done (Top left) |
|  | Under Notifications, set expires to at least 600Tap the checkmark icon to save the setting when done(Top right)Tap the back icon a couple of times to get back to the dial pad. |

|  |  |
| --- | --- |
|  | QR code for iPhone |

|  |  |
| --- | --- |
|  | QR code for Android app installation. |